From f6a45ff2a7bf405da58872611c74fd6bab1d6994 Mon Sep 17 00:00:00 2001
From: Philipp Le <philipp-le-prviat@freenet.de>
Date: Wed, 27 May 2020 00:59:00 +0200
Subject: WIP: Chapter 5

---
 chapter04/content_ch04.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'chapter04/content_ch04.tex')

diff --git a/chapter04/content_ch04.tex b/chapter04/content_ch04.tex
index e93f287..6cd3635 100644
--- a/chapter04/content_ch04.tex
+++ b/chapter04/content_ch04.tex
@@ -2146,7 +2146,7 @@ The dynamic range increases, when more bits $B$ are added. However, the number o
 %
 %Analogous to the thermal noise floor,
 
-\subsection{Time Recovery}
+\subsection{Synchronization 1: Time Recovery}
 
 For wideband \ac{RF} applications, the sampling rate is chosen close to the maximum frequency of the signal, so that the Shannon-Nyquist sampling theorem can be fulfilled.
 
-- 
cgit v1.1

