From 81dcd195ac57fd89ef79d02e467e9fa86024b416 Mon Sep 17 00:00:00 2001
From: Philipp Le <philipp-le-prviat@freenet.de>
Date: Thu, 15 Apr 2021 09:08:56 +0200
Subject: Typo fixes

---
 exercise01/exercise01.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'exercise01/exercise01.tex')

diff --git a/exercise01/exercise01.tex b/exercise01/exercise01.tex
index a92da97..efaaadf 100644
--- a/exercise01/exercise01.tex
+++ b/exercise01/exercise01.tex
@@ -64,7 +64,7 @@
 \end{solution}
 
 \begin{question}[subtitle={Frequency Allocation}]
-	An LTE (4G cell phone) signal can occupy a bandwidth of up to \SI{20}{MHz}. One of the bands allocated to LTE is, amongst others, the band 1 (uplink: \SIrange{1920}{1980}{MHz}, uplink: \SIrange{2110}{2170}{MHz}). The range of one LTE base station is a few kilometres.
+	An LTE (4G cell phone) signal can occupy a bandwidth of up to \SI{20}{MHz}. One of the bands allocated to LTE is, amongst others, the band 1 (uplink: \SIrange{1920}{1980}{MHz}, downlink: \SIrange{2110}{2170}{MHz}). The range of one LTE base station is a few kilometres.
 	
 	However, the HF band (\SIrange{3}{30}{MHz}) has the advantage that waves are reflected by the ionosphere and can propagate over longer distances or even across the whole world. Mostly, narrow-band services like AM broadcasting or amateur radio are allocated to the HF band.
 	
-- 
cgit v1.1

